

**30,000-Gallon Storage Vessel**

**Vineland, NJ**

**VESSEL SPECIFICATIONS**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Manufacturer** | **Year** | **Capacity**  **(Liquid Gallons)** | **PSI**  **(@ 125 °F max.)** | **National Board Number / Serial Number** |
| Trinity | 1995 | 30,000 | 250 | 121677 / 82960 |

The vessel listed is ASME certified and was manufactured by Trinity Industries. It has a National Board number with a U-1A data sheet. This steel vessel is 109- inches in diameter and 66- foot in length. Its shell sections are .437” thick and made from SA-612 steel. Its hemispherical heads are .437” thick and constructed of SA-455 steel.



